**Kanalliste exportieren**

**Stecken Sie die U-Stick in den USB-Anschluss→Suchen Sie alle Kanäle→Rufen Sie das Werksmenü auf（Drücken Sie "SOURCE2580" auf der Fernbedienung）→Benutzer→Werksprogramm-Voreinstellungsfunktion→Exportieren Sie die DVBS-Voreinstellungsdatei nach→Erfolgreich.**

 



**Edit channel list**

Install the “Edit Tool” onto PC desktop and open it.



**1.Inport**

Click the Inport to inport the “preset dvbs\_channels.xml” file, as below picture,After inport the file, you can edit each channel directly



1. **Clear**

If you want to discard the XML change and start over, Click Clear directly.

**3.Move Up/Move Down**

Click on the sub-attribute position of any row, and then operate Move Up to exchange the entire item content with the previous row of the same type, as below picture; In the same way, you can click on the sub-attribute position of any row, and then operate Move Down to exchange the entire item content with the next row of the same type, as below picture.





**4.Channel Swap**

You can directly enter the ch\_num attribute value of the two items that need to be exchanged by selecting the program type, and then click Channel Swap to exchange all the contents of these two items, as below picture.



**5.Delete**

You can select any row of item content, click Delete to delete the row content,as below picture show. 

**6.Sort**

Regardless of whether the ch\_num of each entry in the xml file is arranged in order, just click Sort to arrange the ch\_num of the same type of programs in the order of 1 2 3 4..., please see below pictures





**7.Export**

After editing the xml file, you can click Export to export the new xml file. If the export is successful, there will be a prompt menu, as . The exported xml file will replace the original imported xml file.



**Load channel list:**Copy the final channel list into U dish→Insert U dish to USB port→Auto Search→Preset Scan









